If the pigpio daemon is running it should be killed (sudo killall pigpiod) before make install and restarted afterwards (sudo pigpiod).
The initial part of the make, the compilation of pigpio.c, takes 100 seconds on early model Pis. Be patient. The overall install takes just over 3 minutes.

### Download and install latest version

`wget https://github.com/joan2937/pigpio/archive/master.zip
unzip master.zip
cd pigpio-master
make
sudo make install
`
If the Python part of the install fails it may be because you need the setup tools.
`sudo apt install python-setuptools python3-setuptools
`

### To check the library

These tests make extensive use of GPIO 25 (pin 22). Make sure nothing, or only a LED, is connected to the GPIO before running the tests. Most tests are statistical in nature and so may on occasion fail. Repeated failures on the same test or many failures in a group of tests indicate a problem.
`
sudo ./x_pigpio # check C I/F
sudo pigpiod # start daemon
./x_pigpiod_if2 # check C I/F to daemon
./x_pigpio.py # check Python I/F to daemon
./x_pigs # check pigs I/F to daemon
./x_pipe # check pipe I/F to daemon
`

### To compile, link, and run a C program

`gcc -Wall -pthread -o foobar foobar.c -lpigpio -lrt
sudo ./foobar``
`

### To start the pigpio daemon

`sudo pigpiod
`

### To stop the pigpio daemon

`sudo killall pigpiod
`

### github

`git clone https://github.com/joan2937/pigpio`

### Raspbian (raspberrypi.org image)

This may not be the most recent version. You can check the version with the command pigpiod -v.

`sudo apt-get update
sudo apt-get install pigpio python-pigpio python3-pigpio`